en

conf t

host R1

Int f0/0

Ip address 192.168.1.1 255.255.255.0

No shutdwon

Exit

Ip dhcp excluded-address 192.168.1.1

Ip dhcp pool VOIP

Network 192.168.1.0 255.255.255.0

default-router 192.168.1.1

Option ?

Option 150 ip 192.168.1.1

telephony-service

Max-dn 2

Max-ephones 2

ephonIp source-address 192.168.1.1 port 2000

Exit

ephone ?

ephone- dn 1

number 10

exit

ephon-dn 2

number 20

exit

ephone 1

button 1:1

exit

ephone 2

button 1:2

exit

show ephone

dial-peer voice 1 voip

destination-pattern ..

session target ipv4: 10.10.10.2

😊 🙁